# Changelog

## 0.2.0 — Bayou Radar Primary Data Architecture

- Made `backend.bayouradar.com` the primary weather-alert source.
- Added support for Bayou Radar point and bounding-box alert routes.
- Added direct NWS fallback only for monitored areas whose Bayou Radar request fails.
- Treated a valid zero-alert Bayou Radar response as authoritative.
- Added flexible normalization for GeoJSON and Bayou Radar alert-list payloads.
- Added UGC filtering when the Bayou Radar payload supplies affected-zone metadata.
- Preserved unexpired cached alerts when both sources fail for an area.
- Added per-area source routing, primary health, fallback areas, and last primary success to status JSON.
- Updated the Bayou Radar dashboard with live data-source routing information.
- Moved new configurations to a shared top-level `areas` section while retaining compatibility with `nws.areas`.
- Added automated tests for empty primary responses, payload normalization, invalid primary data, full fallback, and partial per-area fallback.

## 0.1.1

- Centered all public product language on Bayou Radar and its weather-intelligence mission.
- Updated the local dashboard and documentation.
- Removed obsolete migration components.

## 0.1.0

- Initial clean service-based release for Asterisk/app_rpt weather-alert automation.
